| Clause | Remarks/Guidelines |
| --- | --- |
| NTT C22 Provision of temporary electricity and water supply to \*Working Areas/\*Site | |
| [Version A]  Tenderers’ attention is drawn to Particular Specification Clause [X]# on provisions of electricity and water supply to the \*Working Areas/\*Site and the application arrangement for temporary electricity and water supply.  or | Please refer to DEVB TC(W) No. 13/2020.  \* Delete/Modify as appropriate.  # Insert appropriate reference.  Version A – for situation that cables/water mains laying works for electricity and water supply are anticipated to be completed before the scheduled date of site possession. |
| [Version B]  Tenderers should note that the *Client* has already made applications and settled the respective fees for the supply of temporary electricity and water supply to the \*Working Areas/\*Site, with details as more particularly set out in Appendix *[see below]*.The electricity cable and water mains laying works are in progress*.* | Version B – for situation that cables/water mains laying works for electricity and water supply may not be able to be completed before the scheduled date of site possession. |
| Appendix […]   1. Electricity cables and water mains under the applications by the *Client* will be laid up to the boundary of \*Working Areas/\*Site, including WAXX and WAYY [To insert identification of sites concerned]. The electricity load and size of water mains to each of these \*Working Areas/\*Site being applied for are set out in the tables below and the respective alignments and connection points are shown in Plan(s) XX [To insert layout plans showing the indicative cable and water main alignment].  |  |  | | --- | --- | | \*Working Areas/Site | **Temporary electricity load**  **(Amp)** | | e.g. WAXX | e.g. 400 | | e.g. WAYY | e.g. 400 |  |  |  | | --- | --- | | \*Working Areas/Site | **Size of water mains**  **(Nominal diameter in mm)** | | e.g. WAXX | e.g. 200 | | e.g. WAYY | e.g. 100 | |  |
| 1. Upon completion of laying the electricity cables, the *Contractor* shall submit an application to the respective power company, together with a written authorization letter, if required, issued by the \**Project Manager*/\**Supervisor* authorizing the *Contractor* to make use of the relevant connections for temporary electricity supply to the \*Working Areas/\*Site. |  |
| 1. The *Contractor* shall submit an application1 to the Water Supplies Department, together with a written authorization letter, if required, issued by the \**Project Manager*/\**Supervisor* authorizing the *Contractor* to make use of the relevant connections for temporary water supply to the \*Working Areas/\*Site. | Note 1: WSD accepts application from the Contractor before completion of water mains laying works. |